**Shed**

* Replace bottom two back boards with 2 pieces of the 9 inch architrave
* Replace the band all around the top with the straight edge timber.

**Front Door**

* Plinth

**Kitchen**

* Box in top pipe with screw access
* Box in bottom pipe with screw access
* Fit Glass in kitchen doors
* All doors and shelving units to be added
* Dishwasher and appliances to be added
* Hang Door
* Fit lock and escucions

**Hall**

* Skirting
* 2 x Radiator Covers
* Cover wiring inside in the under the stairs cupboard on the Right Hand Side

**Living Room/Dining Room**

* Skirting
* Fit Picture Rail
* Hang doors \* 2
* Fit door knobs and escuscions \*2

**Downstairs Loo**

* Hang Cloak hanger on door

**Stairs**

* Fix stairs where parting
* Add bracket at top of stairs

**Hot Press**

* Fit Shelf (use the straight pieces of primed timber)
* There is a hole on the front bottom right. Would a short piece of skirting look better there along the front as it could be painted. Plywood would not look good with carpet

**Small back bedroom**

* Have a look at knob it’s very tight
* Fit wooden floor

**Bathroom**

* Hang Cloak hanger on door
* Fit inside lock

**Landing**

* Finish panelling

**Middle Bedroom**

* Hang door
* Fit lock and Escucions

**Ensuite**

* Fit inside door lock (toilet)
* Hang bedroom Door
* Hang Cloak hanger on door
* Fit lock and Escuscions