# Asda

## A

# Asdf

# 3asdf

## Electrical

### Front Ground Floor

|  |  |  |
| --- | --- | --- |
| Location | Defect | FYI |
| Wall Adjacent to 101 | Double socket box, detached from box & misaligned, screws missing | Secure with matching screws |
| Wall adjacent to street | Socket unlevel |  |
| All (Double sockets) | Non matching screws | Replace current with matching screws |

### Rear Ground Floor

|  |  |  |
| --- | --- | --- |
| Location | Defect | FYI |
| Wall Adjacent to 101 | Tv Box loose | Fix |
| Wall adjacent to 101 | Double socket detached from box, misaligned & cover not screwed, screw missing | Secure with matching screws |
| All (Double sockets) | Non matching screws fitted &some missing | Replace current with matching screws |

### Hall

|  |  |  |
| --- | --- | --- |
| Location | Defect | FYI |
| Light fitting under center piece | Loose ceiling rose | Fix |
| All (Double sockets) | Non matching screws fitted | Replace current with matching screws |

### Kitchen

|  |  |  |
| --- | --- | --- |
| Location | Defect | FYI |
| Adjacent to French Doors | Tv Box & Double socket unlevel |  |
| Over worktop to the right of hob | Double socket not screwed, screws missing | Fix with matching screws |
| Over worktop to the right of sink | Double socket unscrewed with face marked | Tested available short screws which secured the remaining worktop sockets. These screws did not fit this socket.  Socket cover marked.  Replace the cover and secure. |
| Adjacent to 103 at rear | Double socket & TV point unlevel |  |
| All (Double Sockets) | Non matching screws fitted & some missing | Replace current with matching screws |

### Rear Bedroom

|  |  |  |
| --- | --- | --- |
| Location | Defect | FYI |
| Rear | Inadequate & crooked gap left between socket and tv box | Fuse both together & fill gap to RHS |
|  | Double socket - screw missing | Secure with matching screws |
|  | Light switch unlevel |  |

### Lower Landing

|  |  |  |
| --- | --- | --- |
| Location | Defect | FYI |
|  | Immersion switch and light switch unlevel |  |

### Bathroom

|  |  |  |
| --- | --- | --- |
| Location | Defect | FYI |
| Light over rear of bath | Downlight not lighting | Assess connection/fitting/bulb |
|  | Wall light not fitted | Fit |

### Middle Bedroom

|  |  |  |
| --- | --- | --- |
| Location | Defect | FYI |
| Chimney breast | Tv Point and double socket both unlevel |  |
| Internal Wall | 2 x double sockets unlevel |  |

### Upper Landing

|  |  |  |
| --- | --- | --- |
| Location | Defect | FYI |
|  | Double socket - unlevel |  |

## Master Bedroom

|  |  |  |
| --- | --- | --- |
| Location | Defect | FYI |
| Wall adjoining 103 | 2 x Double socket - unlevel |  |
| Ensuite | Wall light not fitted | Fit |

## Exterior

|  |  |  |
| --- | --- | --- |
| Location | Defect | FYI |
| Left of French Doors | Cable hanging loosely | Conceal in matching black cable tidy/trunking. |
| Shed | Switch–screw missing | Secure |